**How to clean open fit tubes**

1. One type of tubing unscrews and the other can be pulled off. Ask the

Audiologist which type you have.

2. Give the end, which is a dark grey or white dome, a clean with a wet wipe or a tissue. Be very gentle to make sure you do not loosen or remove the dome.

3. Use the cleaning wire as pictured in the diagrams below:



Push the cleaning wire through the top

Pull wire completely through the dome and remove

4. Attach the tube back by pushing or screwing back onto the hearing aid. Ask the Audiologist which type you have.

**How to insert open fit hearing aids**



1. Make sure the battery drawer is open, which means the hearing aid is turned off. Place the hearing aid over the top of your ear.



2. With your index finger, follow the tubing down from the hearing aid to where the tip is. Then push the tip down into ear canal as far as you can/as far as it is comfortable.



3. Curl the retainer wire into the bowl of the ear and close the battery drawer. You have now completed insertion.



4. This is how it should look from the front; the tubing should be flush to the ear. We recommend you practice this as much as you can, preferably in front of a mirror.